Ecology response for DC/22/93828 Land at Villeneuve St George Way, Eastleigh, SO50 9SJ
Construction of a car dealership (Class Sui Generis), incorporating a workshop, ancillary offices, associated parking, access, servicing, landscaping, access, and other associated works
Rebecca Altman
Original application was F/21/91786
Refer to discharge of conditions 13 and 14 (drainage and drainage maintenance) - Construction of a car dealership (Class Sui Generis), incorporating a workshop, ancillary offices, associated parking, access, servicing, landscaping, access, and other associated works
	13


	Development shall not commence until an updated Drainage Strategy has been submitted to and approved in writing by the Local Planning Authority.  The Drainage Strategy shall include full details of the mechanisms for filtration including pollution mitigation indices.  The Drainage Strategy shall thereafter be implemented fully in accordance with the approved details.  

Reason: To ensure that drainage of the site is properly managed in the interest of amenity, to prevent flood risk and to prevent pollution to Monks Brook, a tributary of the protected waters of the River Itchen.  
 


	14


	Prior to occupation and operation of the development hereby permitted, details for the long-term maintenance of the drainage system shall be submitted to and approved in writing by the Local Planning Authority.  The details shall include: 
· Maintenance schedules for each drainage feature type and ownership; and
· Details of protection measures.
The drainage system shall thereafter be maintained in accordance with the approved details. 

Reason: To ensure long term maintenance of the drainage system to prevent flood risk to the site and surrounding area. 
 
3/10/22

The following documents were relevant to the discharge of condition 13: 


Proposed Drainage Layout (Rev P6, September 2022) 114334-CAL-XX-XX-DR-D-0002
Proposed Drainage Schedules (Rev P4, June 2022) 114334-CAL-XX-XX-DR-D-0003
Proposed External Works Layout (Rev P3, September 2022) 114334-CAL-XX-XX-DR-D-0010 and -0011
External Works Construction Details (Rev P3, June 2022) 114334-CAL-XX-XX-DR-D-0600
The Hydro Up-Flo filter using the Simple Index Approach by Hydro International
The surface water treatment train is clearly shown on the proposed drainage layout. 
Condition 13 can now be discharged. 
There were no documents submitted that contained details for the long-term (or any) maintenance of the drainage systems. These are required to be reviewed for Condition 14. 
Lisa Malter
Ecologist











