Ecology response amended for F/22/93437 6 GROSVENOR ROAD SO53 5BW
Demolition of existing bungalow and construction of 1no. five-bedroom 2 storey dwelling with associated landscaping
Alex Webb/Rachael Morris
17/10/22
A functioning soakaway on already site means that no additional testing is needed. The architect has confirmed that there is a functioning soakaway on site which has been signed off by Building Control. I have no further concerns. 
Lisa Malter

25/8/22
I have reviewed the DAS by Crafted Architects and the Preliminary Bat Survey by 4Woods Ecology (June 2022).
The bungalow to be demolished has negligible bat roost potential. The proposals for biodiversity enhancement recommended in the report are suitable and should be implemented. These are a bird box installed on the mature tree in the rear garden, existing garden planting to be supplemented with x10 plant species considered to be of value to pollinating insects and a sedum roof on part of the rear flat roof of the new dwelling. Night flowering scented plants will attract moths as food for bats. 
The surface water drainage proposals of a sedum roof, a rainwater harvesting butt and soakaways are suitable if soakaways were used in the existing bungalow. If soakaways were not previously used on site, then an infiltration test is required. Soakaways must be located at least 5 m from any structure. The size of the soakaways can be determined by the building inspector. The rainwater harvesting water butt overflow should enter the surface water drainage system. 
Lisa Malter
Ecologist



