March 2023 
Water’s Edge Construction and Environment Management Plan
The following measures will be put in place during the construction phase of the development:
• The site manager and all site operatives will be made aware of the presence of the River Hamble and the requirement to ensure it is safeguarded at all times from construction impacts such as noise and visual disturbance, water pollution and dust.
• All excavation associated with the building of the pool will be hand-dug.  Heavy machinery cannot access the site.  Therefore, this should minimise disturbance to overwintering birds that feed and roost in the area, as the proposed level of activity is within the existing normal parameters for the area.
• The spoil dug out to form the pool will be re-distributed evenly across the existing garden.  The modified ground height will not exceed the height of the existing retaining wall adjacent to the River Hamble at any stage.  Therefore, run-off with elevated sediment loading from the site entering the River Hamble should be minimal.
• Any temporary site compound set out for the storage of equipment and materials associated with the construction works will be located as far from the River Hamble as possible and not within 10m of the Mean High Water line.  All stockpiles of loose material will be covered to prevent run-off during periods of rain or wind dispersal of dust. Any temporary compound and all associated construction materials will be removed on completion of the works.
• During excavations, soil will be sprayed with water to prevent wind pick-up.  Stone cutting will be water sprayed to minimise dust drifting and will take place within a screened area situated as far inland as possible and not within 10m of the Mean High Water line of the River Hamble to reduce disturbance to birds. 
• Construction will take place during daylight hours only, therefore, temporary construction lighting will not be required.
• A timber escape ramp will be placed in any excavation overnight or when left for long periods of time to prevent animals becoming trapped.  In addition, all pipework will be temporarily plugged/capped when left unattended to prevent entrapment of or habitation by animals.  


