DC/23/94783 Land between Burnetts Lane and Allington Lane,
Discharge of Condition application for Condition 3-Final Surface Water Drainage and Condition 20 Watercourse Buffer details of F/21/91185 Construction of road between Allington Lane and Burnetts Lane with associated footway, cycle paths, water crossings, drainage and landscaping
Thank you for consulting Ecology, my observations are as follows:
I note that the LLFA (as the responsible authority) have requested more information regarding exceedance flow plans. The lining of the SUDs is not yet confirmed, although there is provision for lining all features should this be required post-infiltration testing which seems a reasonable approach.  My comments hereafter will be confined to Ecological impacts both on-site and off-site. 
Two RAMS document have been submitted (“K25020 RAMS 5 Rev.A Works in vicinity of watercourses” and “K25020 RAMS 3 Rev A Temporary fluming of streams”) which detail construction phase mitigation measures to protect both on-site and offs-site ecological receptors. The content and scope of the documents is adequate to protect the receptors. It should be noted that ongoing monitoring and the role of the Ecological Clerk of Works are essential to ensuring that the measures within the documents are implemented effectively. 
On the basis of the submitted information I recommend that Conditions 3 and 10 can be discharged from the Ecology perspective. All works thereafter to carried out in strict accordance with the details submitted within the RAMs documents and cross referencing the over-arching CEMP that is approved through permission F/21/91185.

Paul Howe MCIEEM
Ecologist
Date 28/04/23
