SPECIFICATION OF WORKS 

Rigden – CQ14393-NA – J7770


T1	Dead Silver Birch

· Sectional dismantle to ground level.

G2	Group of  x 5 Sycamore trees

· Remove x 2 trees with extensive bark wounds at ground level.
· Remove smaller tree leaning towards neighbouring property.
· High pollard of the x 2 remaining trees with asymmetric crowns.

T3	Pedunculate Oak

· Located in neighbours garden.
· Crown lift to 5m by removal of secondary branches only.
· Remove major deadwood.

T4	Larch

· Monitor fungi at ground level to the west.

T5	Large Pedunculate Oak

· Located in the rear garden.
· Remove major deadwood.

T6	Weeping Willow

· Previously pollard.
· Re-pollard to just above pollard points.


REASON – SOUND ARBORICULTURAL MANAGEMENT
