Chalcroft Business Park, Burnetts Lane
RM/23/94868 Two building solution
Landscape comments: Mark Ellison 31/10/23
Landscape Plan:  DD614L05
1. Can we change the two Field Maple trees along the frontage to Elms please so that we’re establishing a cohesive avenue. 
2. Please reduce the footway in front of the buildings to 1.8m wide, which would enable a 0.2m wide increase in the adjacent planting beds.1
Planting details Plan 2 : DD614L02
1.For clarity’s sake please add in the planning application reference to the title block or refer to a ‘two building solution’.
2.  Please identify the nature of the existing and imported topsoil. If its pretty free draining I don’t think the new level of the tree needs to be raised. Also, I’m still uneasy about a layer of new topsoil that is only 300mm deep. Please amend the drawing to state that it should be 450mm minimum for areas within existing hardstanding and 300mm in existing areas of grass, although happy to debate this with the landscape architect if I’ve missed some new evidence. In the areas where trees are able to be planted within areas of existing grass, no imported subsoil will be required.
3. In my previous comments I wrote;
‘In relation to the tree stock size we usually require a minimum of 14-16cm girth. However, in the circumstances of this site and because the client has appointed a trusted local landscape firm we are happy to compromise on this with the following condition;
That the developer funds the landscape architect to visit Hilliers nursey in Liss or Ampfield to select the trees individually. In doing this it is usually possible if this is done early enough to select specimens that are at the top of the size range and also of a good balanced shape, with a strong leader and no wounds. If this is guaranteed then we’d be happy to accept the stock sizes specified.’
I understand that the client for the project is happy for this to happen, but the latest submission doesn’t recognise this. Can the applicant please re-submit the LEMPs with a statement that this is what will happen. In the overing email, please let us know where in the LEMPs you’ve included this. 
Under BS 3882: 2015 one is obliged to designate the type of topsoil. I suggest you specify 
‘multipurpose’.
