DC/23/96596 Fair Oak Sport Pavilion
Ecology comments 3.1.24

Condition 4 LEMP
The submitted Landscape Management Plan is now fine.

Condition 6 Pitch drainage
Drainage for the new wetland area at the SW of the site
Outlets: The proposed height of each overflow channel from the new wetland area is shown but the width of them is not.  Please can this be shown.  The width of the overflows should be wide enough to allow low energy, sheet flow discharge to reduce the likelihood of an incised channel forming at the downstream end of either overflow and therefore reduce the impact of any discharge on the adjacent habitat.
Inlet: Drainage plan Tgms1111.12-4 Phase 2 Drainage Design indicates an inlet at the north of the new wetland area.  Please could text be added to make this feature clear and for consistency could this feature be also shown on the cross-sections plan -6 and catchment plan -9.  This demonstrates that all the drainage from the existing collector drain serving the catchment shown on the catchment plan -9 is intercepted and discharged into the new wetland feature.  Therefore, the new wetland will capture as much run-off as is pragmatically available.  It is acknowledged that the inlet shown may not be the inflow mechanism delivered on the ground as this will be dependent on the levels of the base of the new wetland in relation to the level of the existing collector drain but the effective outcome (maximum capture of run-off into the new wetland) must be the same. 
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