Design and Access statement 

Must have a new gas boiler for heating and hot water and this requires a new flue pipe that will have  a slightly increased size of guard (circa 10mm). This also requires a 40MM condenser pipe on external wall coming out at 150mm above ground level and going down.
