
H/26/101344
Installation of a pair of driveway gates, a pedestrian gate and associated brick piers (amendment to H/25/100267 to alter size and set-back of gates).


Driveway Gates
Proposed materials and finishes:
A pair of matching driveway gates, filling a 3.6m gap, opening inwards towards the house and mounted on the rear (house side) of the pilers. 2m high, rising to 2.2m in the centre.
Gate frames are grey and made from marine-grade anodised aluminium. The composite slats are made from premium eco-friendly recycled materials and have a grain finish to resemble wood and are Teak colour, with a matching pedestrian gate.
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