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Introduction

This Construction Environment Management Plan (CEMP) has been produced to accompany the planning application (ref. F/24/97883) for ‘Mounding works and the relocation of the existing vehicular access to the play area and paddling pool’ at Fleming Park Play Area, Passfield Avenue, Eastleigh.

Both parties to the preparation of this report have much successful experience of delivering earthworks without creating local nuisance. It is also noted that this development involves the movement of only a relatively small amount of material (approximately 750m3). This is anticipated to be completed with two weeks of work on site. Please also refer to the planning drawings.

a) The location of temporary site buildings, compounds, construction material and plant storage areas used during demolition and construction

Any temporary site buildings etc will be located to minimise disruption to the use of adjacent public areas. Note that for most of the contract period the paddling pool and play areas will be closed to public use for safety reasons. It is anticipated that the only temporary building will be a small welfare / office unit for the site operatives.

b) The arrangements for deliveries associated with all construction works, loading/ unloading of plant & materials and restoration of any damage to the highway [including vehicle crossovers and grass verges]. 

The existing vehicle access and the proposed new access will enable vehicular access without the need for crossing on grass verges. The size of the development would not be appropriate for large numbers of vehicles and the lorry movements per day will be minimal so as not to cause queueing on Passfield Avenue. It is anticipated that only ~75 HGV loads of soil would be required to complete the project.

c) The parking of vehicles of site operatives and visitors

Where possible all site staff vehicles will be parked within the site, accessed by the existing vehicular access from Passfield Avenue. This is a small engineering project that will require very limited staff and therefore limited parking. For site meetings the car park at Places Leisure can be used for parking. 
d) Measures to control the emission of dust and dirt generated by demolition and construction

The works are not planned to start before the second week in September when there is a good chance that there will be sufficient rain to reduce the risk of dust nuisance, but not enough to pose a high risk of mud being tracked onto Passfield Avenue and surrounding hard surfaces. Nevertheless, the following, measures will be taken to control dust.

Works will temporarily be suspended during weather conditions that would cause excessive dust generation. Circumstances that are likely to lead to a suspension in operations could include dry conditions with a high wind speed where the use of plant and machinery is generating large dust volumes that are visibly being carried beyond the boundary of the development site.

The prevailing winds, as measured at the nearby Southampton Airport are principally from the south-west and to a lesser extent the west and south. Whilst this reduces the risk of dust pollution effecting the river to the west of the site, it suggests that the following are at risk:

· Passfield Avenue 
· Houses to the east of the site
· Shell petrol station to the north-east

There is an intermittent line of mature trees along the site boundary that will to some degree mitigate the risk of dust pollution to the above. Whilst the nearest houses are around 20-30m from the nearest edges of the earthworks, most of the imported soils would be contained withing the proposed new mound to the northwest of the paddling pool. Taking a measurement along the SW/NE alignment of the prevailing wind the nearest houses are approximately 100m away.

The paddling pool and play areas closest to the site will be closed during the main part of the earthworks.

On that basis we have a high degree of confidence that dust control measures employed on site would be effective in mitigating the effects of dust generation and that receptors would experience no greater than a negligible effect from dust impact. However, in addition to the stopping or work during high winds the following measures will be taken by the contractor:

· Limiting the height of stockpiles of stripped and imported soils to 4m.
· Damping down of stockpiles.
· Enforcing a 10mph speed limit for HGVs when travelling on site.
· Ensuring all HGVs are sheeted. 
· Ensuring all vehicles switch off engines when stationary.
· Undertaking frequent visual checks.

Upon completion of the earthworks the mounding will be sown immediately with grass seed to cover the exposed area, with planting occurring on completion of all works.

e) a scheme for controlling noise and vibration from demolition and construction activities

There will be no use of vibratory plant during the earthworks phase. This is a small earthworks project requiring the limited and temporary use of plant and machinery on site. There would be no use of plant and machinery before 08:00 (Monday – Friday) and no works at weekends. 

f) Provision for storage, collection, and disposal of waste from the development during construction period

The only significant waste generated on site will be the excavation of existing tarmac. This is only expected to amount to a maximum of 2 HGV loads of waste for exportation. The waste will be loaded directly onto lorries operated by a licenced waste carrier and deposited at an appropriately licenced waste management facility.

g) Measures to prevent mud and dust on the highway during demolition and construction

The tarmaced areas will be regularly swept to ensure they remain clean and that HGVs do not track mud or dust on their wheels. The regularity of sweeping shall be dependent on factors including prevailing weather conditions and intensity of use and shall fall under the responsibility of the site manager.

Site plant and machinery shall be jet washed if necessary to remove any accumulated mud or dust from their wheels or tracks.  A road sweeper shall also be employed to ensure hard running surfaces within the site and the public highway in the vicinity of the site exit and entrance are kept clean.

h) The erection and maintenance of security hoarding 

Herras fencing will be used on site and maintained to prevent public access where appropriate.

i) Temporary lighting

This will not be any temporary construction lighting required. Site works would be limited to hours of daylight only.

j) Protection of pedestrian routes during construction

For most of the contract period the paddling pool and play areas will be closed to public use for safety reasons. The area closed will vary during the project to minimise inconvenience to the public.  

k) Safeguards to avoid pollution on Monks Brook or damage to riverside vegetation

Specifically, to protect the adjacent watercourse Monks Brook from the egress of silty/muddy water flowing from the earthworks silt fencing will be installed. This will prevent sediment from the imported soil being washed into the watercourse by surface water run-off during any periods of rainfall during the work. Upon completion of the earthworks the mounding will be grass-seeded to bind the soils. The silt fencing will remain in place until grass cover has been established. 

It is anticipated that the earthworks nearest the river will be constructed from within the area of railings surrounding the paddling pool (i.e. on the opposite side of the railings from the river). This will avoid any damage to riverbank vegetation. The railings are approximately 5m from the edge of the watercourse. Should access be required from the river side of the railing this can be achieved by means of the existing tarmac path without the need to track over the bankside vegetation. 

l) Hours of working

All works will be limited to 07:30 – 17:00 Monday – Friday. There will be no operations at weekends. There would be no operation of plant and machinery before 08:00.

m) Type of plant to be used 

It is anticipated that the works would principally be completed through the use of a single 360 excavator that would be utilised to place and shape the imported soils. There may a limited requirement for a small bladed dozer for shaping work which will be determined by the site manager during the course of the works.

n) Soil Quality Protocol Pre-Authorisation

The soils needed to complete the earthworks would be clean and inert and imported to site under a U1 Waste exemption: Use of waste in construction as regulated by the Environment Agency. This permits the use of up to 1,000 tonnes of inert soil for landscaping / construction works. All soils would be tested prior to acceptance to ensure they comply with the relevant waste classification.

Alternately, if deemed necessary or appropriate, the project could also be completed under the Definition of Waste: Code of Practice (CL:AIRE), also as regulated by the Environment Agency and the Local Authority. This uses a Materials Management Plan to authorise the movement of suitable soils from one construction project where there is a surplus requiring removal (e.g. at a greenfield housing development) to another construction site where there is a need. 

Under the Code of Practice, the source materials will be subject to characterisation testing and analysis to ensure it is suitable for the proposed use. This will include:

• Review of Site Investigation reports, Soil Analysis/Testing Certificates, previous site history etc.
• The process producing the imported material e.g. bulk excavation and location of soils relevant to existing reports. 
• The Composition of the import material. 
• Volume and dates the material is expected from the Producer/Donor site.
 • Visit(s) to the Producer/Donor site to inspect material as required to assess the appearance of the import material (including its smell, colour, consistency and physical form). 
• Confirmation of the Waste Carrier and the Waste Carrier licence details. 
• Verification that source material meets agreed Soil Import Values.

o) Response to complaints
In the event that a complaint regarding nuisance or adverse impacts to amenity is received, it will be promptly and thoroughly investigated. Where necessary, appropriate remedial actions will  be implemented without delay.
