Design and access statement


I would like to replace the white rough cast and the two triangles under the gable ends with vertical black clic cladding. The link below is the brand and product. Its is a cement fibre board with a fire safety classification  of  A2-s1, d0
I would also like to replace the gable ends with matching new black ones.

The shop sign will also be replaced for the same size but with LED lighting behind it.

I would also like to spray paint the existing UPVC doors and windows at the front black. 

The sides and the back of the building will remain as it is. 

https://www.cedral.world/en-gb/cladding/our-products/cedral-click/


