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Marina Drive Hamble -Le- Rice
Planning  and heritage statement 
Author of report -Alan Cotterill 
Date 12-2-26
Introduction 
Berkeley Homes built the  above development approx. 25 years ago . The works included building 14no houses along with parking . There were some road improvement works involving making the entrance to Marina Drive wider . This was carried out by demolishing dilapidated  brick retaining wall and constructing new log retaining wall with wall pushed back slightly to create  easier vehicular access on marina Drive / Satchell Lane junction 
Below extract from original construction drawing. Log retaining wall highlighted in red 
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Proposed remedial works to estate roads 
We are proposing to carry out remedial works to the estate roads following consultation with the estate management team and the residents . We have produced a detailed scope of works for road and drainage defects . We are currently  obtaining quotations from sub-contractors to carry out the remedial works  and will be placing orders shortly . Part of the defects works is to replace  log retaining wall . We believe  the replacement wall will require planning permission. 
Please note there is a separate planning application to carry out some tree works in the same area . The application submitted by the residents .  

Below drawing showing existing and proposed elevation (The replacement  wall is approx. 22m long ) 
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Below defects identified 
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Description of work that requires planning permission 
Replacement of log retaining wall  on one side of Marina Drive with timber sleepers and steel posts . The log retaining wall needs replacing due to  age approx. 30years old .  Refer to photos of existing log retaining wall 
Image below  showing photo of proposed railway sleeper/steel retaining wall 
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Location plan of development Berkeley Homes built approx. 25 years  
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Below site plan of development . The proposed sleeper wall highlighted in green . 
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Below photos of existing log retaining wall 
Photo 1 
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Photo 2 [image: ]
Photo 3 
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Photo 4 [image: ]
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