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THEO SIMS-HARRIS
ARENA OFFICE,
GROSVENOR HOUSE
BASING VIEW
BASINGSTOKE
RG21 4HG 



	Application  
	DC/25/99595

	
	Please ask for
	Gregg Chapman

	
	Direct dial
	023 8068 8236

	
	Email
	gregg.chapman@eastleigh.gov.uk

	
	
	

	20th April 2026
	
	



Dear Mr Sims-Harris
	
Town and Country Planning Act 1990
Planning (Listed Buildings and Conservation Areas) Act 1990 

In pursuance of their powers under the above Act and in accordance with your application received on 23 June 2025 and made valid on 24 June 2025, the Council, as Local Planning Authority hereby confirm the status of the following conditions in respect of:

	Application No: 
	DC/25/99595

	Description:	
	Discharge of Conditions 10 (Noise), Condition 11 (Dust Assessment and Mitigation), 13&14 (Tree Protection and Arboriculture Method Statement), 15 (Levels), Condition 16 (Pedestrian Link Construction Detail), Condition 17 (Invasive Plant Assessment), Condition 18 (Habitat Enhancement and Management), Condition 19 (Lighting), Condition 20 (Remediation), Conditions 23 and 24 (Foul and Surface Water Drainage), Condition 25 (Noise Mitigation) and Condition 31 (Acoustic Barriers) of Outline Planning Permission O/18/82750 (Outline application for the demolition of existing buildings and erection of 23 employment units (up to 5,905 sq.m.) with units 12-20 for Use Class B1 (b) and (c) and units 1-11 and 21-23 for Use Class B2, with associated car parking and access. Detailed matters considered: Access and layout) approved March 2021.

	Site:
	Land at Netley Firs,  Kanes Hill, SOUTHAMPTON, SO19 6AJ



	Condition
	Details
	Compliance and Date

	24 (Surface Drainage)
	No above ground development shall begin until a surface water drainage scheme for the site, based on sustainable drainage principles, has been submitted to and approved in writing by the Local Planning Authority. The scheme shall subsequently be implemented in accordance with the approved details before development is completed. The scheme shall be based upon the principles within the following documents: 
• 020.5288.001 “Site Layout: Drainage Strategy Sheet 1 of 2” 
• 020.5288.002 “Site Layout: Drainage Strategy Sheet 2 of 2” 
• 020.5288.003 rev B “Drainage Details” 
• 020.5288.004 “Existing Flow Paths” 
• 020.5288.005 rev A “Drainage Design Catchment Areas” 
• Trail Pit Soakage Test Results rec/d 10.12.18 
• Micro Drainage results dated 16.11.18 
• Paul Basham Associates Drainage Strategy Technical Note 020.5288/TN/1, August 2018 
• Paul Basham Associates Drainage Strategy Technical Note 020.5288/TN/2, December 2018 

and shall also include: 
• Further infiltration testing at formation level of the proposed permeable paving areas; 
• Full results of the proposed drainage system modelling for the 1:100 year events plus climate change, inclusive of all collection, conveyance, storage, flow control and disposal elements and including an allowance for urban creep; 
• Detailed drawings of the entire proposed surface water drainage system, including levels, gradients, dimensions and pipe and manhole reference numbers and catchment plans; 
• Full details of the proposed Suds features and any flow control measures; 
• Details of overland flood flow routes in the event of system exceedance, with demonstration that such flows can be appropriately managed on site without increasing flood risk to occupants and third party land; 
• Details of the measures taken to prevent pollution of the receiving groundwater in accordance with the water quality criteria set out in the Ciria SuDS Manual, and 
• Details for the long-term maintenance arrangements for the surface water drainage system (including all SuDS features). 

The submitted details shall identify runoff sub-catchments, SuDS components, control structures, flow routes and outfalls. In addition, the plan shall clarify the access that is required to each surface water management component for maintenance purposes. The maintenance plan shall be carried out in full thereafter. 
Reason: To ensure that the proposed development can be adequately drained and to ensure that there is no flood risk on or off site resulting from the proposed development. 

Documents Submitted;  

MJA Consulting Technical Note - Response to LLFA Consultation (TSH/TN/0040/7230) dated 16th January 2026.
MJA Foul and Surface Water Drainage Technical Note (TSH/TN/0529/7230) dated 19th June 2025.
Surface Water Drainage Strategy - 7230-MJA-SW-XX-DR-C-003 PL7 received 16th April 2026 (amending above)
Hydro International Downstream Defender Advanced Hyrdodynamic Separator received 16th April 2026.


	Approved 
20/04/2026



Where information has been submitted to discharge a condition, any approval given is subject to compliance with the approved details.

Yours faithfully

[image: Text, letter

Description automatically generated]
Nicholas Parker	
Planning Manager
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Eastleigh Borough Council, Eastleigh House, Upper Market Street, Eastleigh, Hampshire SO50 9YN
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