TPO Works Application: Supporting Statement
Property: 7 Corinthian Road, Chandlers Ford, Eastleigh, Hampshire, SO53 2BA
Tree Location: 7 & 9 Peverell Wood Avenue
Tree Species: Mature Oak
Council: Eastleigh Borough Council

1. Proposed Schedule of Works
The applicant seeks consent for the following specific arboriculture operations in accordance with BS 3998:2010:
· Crown Reduction: A reduction in overall height of 3m from the current estimated height of 17.5m, leaving an intended finished height of 14.5m.
· Lateral Reduction: A reduction of the overhanging canopy on the northern aspect by 3m, leaving an intended finished radial spread of 6m.
· Pruning Standards: All work will involve shortening branches to appropriate secondary growth points to maintain a balanced, natural shape and will avoid cutting through the main stem.
· Crown Lift: Lifting of the lower canopy to 4m above ground level.
· Deadwood Removal: Removal of all major dead, dying, or diseased wood throughout the crown. (Note: It is understood that LPA approval is not strictly required for the removal of dead branches )

2. Statement of Reasons
This application is submitted based on the following safety and amenity justifications:
A. Safety and Risk Mitigation
· The tree’s canopy currently encroaches over the applicant’s garden by approximately 9m.
· Directly beneath this canopy is a high-use children’s play area.
· There is a documented history of significant deadwood falling into this play area, posing a direct hazard to residents.
· The proposed reduction is the minimum necessary to reduce "sail area" and mechanical stress on the limbs, minimising the risk of failure over this high-occupancy zone.
B. Structural Integrity and Tree Health
· Reducing the weight on overextended lateral limbs will prevent "end-loading" failure.
· The proposed reduction to recognised growth points ensures the tree’s physiological health is maintained while managing its size in a suburban context.
C. Reasonable Enjoyment of Property
· The 9m encroachment results in near-total shading of the primary amenity space.
· This work seeks a compromise: retaining the tree’s contribution to the landscape while restoring a safe level of light and usage to the garden.

3. Photographic Evidence & Site Plan
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Annotated image showing the proposed 3-4m reduction line to suitable growth points.
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Overall view of the Oak showing the 10m encroachment over the boundary.
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View of children’s play equipment positioned directly beneath overhanging deadwood.
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Sketch plan identifying the tree (T1), the boundary line, and the house


4. Implementation
All works are to be carried out by a suitably qualified and insured arboricultural contractor in full accordance with BS 3998:2010 (Tree Work – Recommendations).
The applicant recognizes the amenity value of this specimen. In accordance with the guidance that the LPA may discuss alternative works:
Should the Local Planning Authority consider the proposed 4m reduction to be in excess of acceptable limits for this specimen, the applicant requests that the Tree Officer propose a modified specification (e.g., a 2m or 3m reduction) rather than issuing a flat refusal. The applicant is fully prepared to discuss a compromise that balances the tree's health with the safety and light requirements of the garden.
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