F/26/101731- Fairport House, Lands End Road, Bursledon, 
                      SO31 8DN.

Context.
This proposal is for a new jetty and pontoon in the most prominent and therefore sensitive position on this part of the river.  It is just round the bend of the salt marshes as one comes upstream on the left bank with a gap of approximately 100m to the next jetty and pontoon and five further ones at 20-30m gaps up to the Jolly Sailor.  The site is within the Old Bursledon Conservation Area and in or adjacent to numerous nature conservation designations.

The Proposal.
The whole structure consists of approximately 17m or 18m (depending on which part of the drawing one takes) of jetty with a bridge or ‘brow’ of 5m connecting it to the pontoon.  Both the jetty and bridge are shown to have handrails either side, but no detail of the material/s or finish, which particularly at low tide, will be the most prominent feature from the land.

These barriers consist of a handrail and mid-point rail with stanchions at approx 1.2m centres.  Private jetty handrails are often of wood, with mild steel, which would need good protection – as the piles – or stainless steel which would glint in the sun are other options.  This would highlight its presence.

Conclusion.
The principle of this structure is not a problem from a built heritage aspect, but the most noticeable element from a landward viewpoint is not detailed.  It either needs to be low key i.e. dark for wood or mild steel or very elegant if stainless steel.
If painted, it both needs to match the piles and be a darker colour to not impose on the headland too much.  Holding objection awaiting handrail details.
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