Page 3  – Specification of works
Turner – CQ14570-NA – J7791

T1	Common Ash

· Located in rear garden.
· Reduce crown by 3.5 m back to secondary Crown
· Remove limb to the east back to stem.
· Remove x 2 low laterals growing towards the property.
· Remove major deadwood.

Reason: Sound arboricultural management.
	


