Page 2 – Specification of works
Watkins – CQ14590-NA – J7793

T1	Pedunculate Oak

· Located in rear garden.
· Reduce lateral spread by 1.0-1.5m to balance crown.
· Selective branch reduction predominantly to the south and west.
· Crown thin by 20%.
· Crown lift to 5.5m by removal of tertiary and secondary laterals only.
· Remove epicormic growth.
· Tidy stubs.
· Remove major deadwood.
· Note crown height to be retained at current stature.
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