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Ref Species Location Notes Work Description

T1 Oak

Rear

garden

T1 is a healthy Oak having had EBC approved (T/20/89203) routine maintenance 

during Spring 2021.  It requires minor routine maintenance to prolong the life of 

the tree and to remove the hazard of falling debris.



Remove epicormic growth.

Remove dead wood from canopy.

T2 Beech

Rear

garden

T2 is a healthy Beech which has greatly benefitted from EBC approved 

(T/20/89203) conservation work carrie out in the Spring of 2021.  However, there 

has been vigorous growth resulting in extended laterals which are now reaching the 

north corner of the property.

Reduce radius by 2.0 metres to provide adequate clearance to the adjacent 

property, maintaining all round shape.

Crown lift to previuosly approved level of 4 metres above adjacent patio removing 

secondary and tertiary branches only.

Pruning wounds to be limited to 30mm maximum.

T3 Oak

Rear

garden

T3 is a healthy Oak located in an elevated position exposing it to unobstructed 

prevailing winds across the Itchen Valley. It benefitted from having EBC approved 

(T/20/89203) maintenance in the Spring of 2021 and only requires minor 

maintenance.

Removal of epicormic growth.

Remove dead wood from canopy.

T4 Oak

Side

garden

T4 is a healthy Oak having had EBC approved maintenance in the Spring of 2021. No maintenance required at this time.

T5 Oak

Side

garden

T5 is similar to T4 and is a healthy Oak. No maintenance required at this time.

T6

Silver

Birch

Side

garden

T6 is an unhealthy Silver Birch showing signs of desease and die back.

It has grown with a strait lean over the adjacent boundary fence and now extends 

approx. 5.5m across the rear garden of the neighbouring property at an angle of 

26 degrees from the vertical, posing a danger to life should it fall.

Cut down and remove.

Schedule of Tree Works – 2 Beechwood Rise, West End, Southampton. SO18 3PW

General Notes:



All works will:

                           • Be undertaken in accordance with British Standard BS3998:2010. Tree Work – Recommendations

                           • Be carried out by a suitably qualified tree surgeon

                           • Seek to retain the natural shape and habit typical of the species

                           • Preserve the special amenity value of the remaining trees, local wildlife and surrounding area


