

Summary of conditions to clear Ref: PP-13478461

Condition 3. CEMP

Find attached HDN Boorley Green CEMP.
We have based our CEMP on the consortium CEMP already in place for the overall development of Boorley Green.
Liaising with the Primary School adjacent and the consortium (developers) managing (Jackson Rowe) who run the public spaces not yet adopted by HCC.

Condition 4 Drainage 

See attached surface water drainage scheme for the site (by Aegaea) , this has been done in conjunction with the new site investigation bore holes carried out in August 2024 by Geo environmental..

Condition 5 Drainage maintenance 

Included within the surface water drainage scheme by Aeagea 

Condition 6. Gas remediation 

See attached report from Geo environmental 

Condition 7, materials 

Brick  - Ibstock Parham Red
Roof covering – Etex cedral Thurtone slate 600 x 300 blue / black.
Windows  - Anthracite UPVC frames 
Class room windows and all external doors – Anthracite Aluminium frames 

Condition 12 Ecological mitigation 

As part of the appraisal KJF carried out a bird nesting report on 9th August 2024 (Nesting Bird Inspection (NBI) on Land adjacent to Boorley Park Primary School, Nairn Road, Botley SO32 2SH), and joint site visit with bore hole site team from Geo Environmental.
Bore hole samples were taken and monitoring over 5 weeks as part of the soil report.

On 3rd September 2024 the vegetation was then flailed to 100mm height as per the appraisal and then strip / reduced in sections and days apart as per the appraisal (after bird nesting season).

Also attached is drawing Eco Enhancements showing locations of habitat / nesting area / animal access points required.




